Dominic Drury

01/17/2024

CS-350

2-2 Milestone One Submission

LAB QUESTIONS

• What does pwmled2 set the PWM period to?

3000 microseconds or 3 seconds

• Which PWM\_xxx() function sets the PWM period?

PWM\_Params\_init()

• Which PWM\_xxx() function sets the PWM duty cycle?

PWM\_setDuty

• What is the purpose of the while(1) loop in pwmled2?

It is a forever loop that increments the PWM duty

• What is the purpose of usleep() in the while(1) loop?

Suspend the execution for 50000 microseconds